**REACH CODE IMPLEMENTATION RESOURCES TEMPLATE**

This template is intended for educational purposes only, without any express or implied warranty of any kind, including warranties of accuracy, completeness, or fitness for any particular purpose. You agree that your use of the template is without any recourse whatsoever to PG&E, SCE, SDG&E, SCG, or their affiliates. The template is a draft, and anyone using this document should seek the advice of an attorney to develop appropriate ordinance language to meet its jurisdiction’s specific needs, as state and local laws may differ.

For additional information contact [info@LocalEnergyCodes.com](mailto:info@LocalEnergyCodes.com)

The IOU Statewide Codes and Standards program is funded by California utility customers and administered by Pacific Gas and Electric Company, San Diego Gas & Electric Company (SDG&E®), Southern California Edison Company and Southern California Gas Company (SoCalGas®) under the auspices of the California Public Utilities Commission and in support of the California Energy Commission.

# Credits

This document is an **abridged version** of the Drought-Ready Construction ordinance developed by Ecology Action, Greywater Action, California Onsite Water Association, and Central Coast Greywater Alliance. This abridged version covers only dual drainage. Full version of the Drought-Ready Construction that covers dual drainage and dual water supply can be accessed at <https://centralcoastgreywater.org/drought-ready-buildings-ordinance/> .

This document is an adaptation of “Greywater Ready Buildings” model ordinance developed by **Laura Allen** (Greywater Action) and **Regina Hirsch** (California Onsite Water Association).

The lead author of this documentis **Sherry Lee Bryan** (Ecology Action, Central Coast Greywater Alliance).

The authors thank the following people for making contributions to this document:

Art Ludwig (Oasis Design),

Brad Lancaster (Harvesting Rainwater for Drylands and Beyond),

Christina Bertea (Greywater Action),

Dakotah Bertsch (Dakotah Bertsch Landscape Architecture),

Golden Love (Love's Gardens),

Jeff Hutcher (Building in California),

John Russell (Water Sprout),

John Scarpulla (San Francisco Public Utility Commission),

Justin Burks (Santa Clara Valley Water District),

LeAnne Ravinale (Scotts Valley Water District),

Leigh Jerrard (Greywater Corps),

Mary Ann Dickinson (Alliance for Water Efficiency),

Osama Younan (Los Angeles Department of Building and Safety),

Paul James (Water ReNu),

Sierra Ryan (County of Santa Cruz), and

Steffi Becking (Energy Solutions on behalf of the California Statewide Codes and Standards Reach Codes Team).

# Drought-Ready Construction Model Ordinance (**abridged version**)

**SECTION 1. FINDINGS AND DETERMINATIONS**

Growing population, climate change, and droughts make it essential for the [City, County, or Water District] to manage its water resources as efficiently as possible.

Reducing the demand for potable water through onsite water reuse improves reliability of local water supplies, reduces impact on downstream wastewater treatment facilities, reduces energy consumption and greenhouse gas emissions, and provides environmental benefits, including protecting water quality and preserving stream flows.

The cost to make dual drainage plumbing accessible for installation of a future graywater irrigation system is lowest during the construction or certain remodels of a bathroom or laundry room when the piping is being installed.

**SECTION 2. INTENT**

The intent of the Drought-Ready Construction model ordinance is to lower the costs and barriers for future installation and future use of graywater irrigation systems by pre-plumbing buildings during construction or during certain remodels that expose drainage piping.

**SECTION 3. DEFINITIONS**

**Diverter valve:** A single valve that can direct graywater to either a sewer/septic system or to a graywater irrigation system.

**Dual drainage plumbing:** Graywater drainage pipes and the necessary connecting pipes, fittings, valves, and all appurtenances carrying untreated graywater to a diverter valve that, on one side, allows the graywater to flow to a blackwater pipe and, on the other side, diverts the graywater to a graywater stub-out.

**Graywater**: Untreated wastewater from bathtubs, showers, bathroom sinks, clothes washers, and laundry tubs. For the purposes of this ordinance, graywater is intended for landscape irrigation or as a source for onsite treated nonpotable water to use for toilet flushing.

**Graywater stub-out:** A capped termination point of graywater drainage piping extending from the diverter valve; typically located outside of a dwelling and ready to be connected to a graywater irrigation or reuse system.

**SECTION 4. APPLICABILITY**

The provisions of this ordinance shall apply to the following buildings:

* New residential construction including accessory dwelling units (ADUs), single-family dwellings, duplex dwellings, and multi-family buildings;
* Bathroom or laundry room addition in ADUs, single-family dwellings, and duplex dwellings;
* Bathroom remodel that alters drainage piping to shower(s) in ADUs, single-family dwelling, and duplex dwellings; and
* Laundry room remodel in ADUs, single-family dwellings, and duplex dwellings.

**SECTION 5. REQUIREMENTS**

1. **Dual drainage plumbing.**
2. Dual drainage plumbing shall be included in new residential construction and applicable additions and remodels so that the graywater can be diverted into a future graywater irrigation system. Dual drainage plumbing shall include readily accessible diverter valve(s) and stub-out(s) and allow graywater to be diverted from graywater sources specified in Table 1.
3. When the location of a diverter valve is not accessible for manual valve operation, an electrical outlet shall be located within 10 feet of the diverter valve so that an electronic actuator can be connected to the diverter valve for remote operation.
4. The graywater stub-out(s) shall be located outside of the dwelling and adjacent to an existing or future landscaped area. The graywater stub-out can also be located in a garage, basement, or mechanical room when site elevations or intended use of graywater requires a pumped system.
5. A dedicated 120-volt electrical receptacle with ground-fault circuit interrupter shall be located within 10 feet of the graywater stub-out(s) so that a pump can be installed for a future graywater system.

**EXCEPTION to Section 5(a)4**: Laundry-to-landscape graywater systems that use a clothes washer’s internal pump to distribute graywater through irrigation distribution piping are exempt.

1. The graywater stub-out(s) shall be permanently marked “CAUTION: NONPOTABLE GRAYWATER, DO NOT DRINK.”
2. Dual drainage plumbing shall meet all requirements in the California Plumbing Code.

**EXCEPTION 1 to Section 5(a)**: Projects with landscaped area within 100 feet from a creek, wetland, river, or located in an area where groundwater is documented less than 3 vertical feet below the excavation of the graywater irrigation field or mulch basin(s), are exempt.

**EXCEPTION 2 to Section 5(a):** Bathroom and laundry room remodels where existing drainage plumbing is embedded in a concrete slab, and where under-slab drainage plumbing is not being altered or extended, are exempt.

**EXCEPTION 3 to Section 5(a)**: Projects with landscaped areas that are unable to infiltrate the daily volume of graywater produced from mandatory graywater source(s) in Table 1 are exempt. Project applicants claiming this exception shall submit documentation demonstrating exception’s applicability.

***TABLE 1:*** *Graywater Sources Requiring Mandatory Dual Drainage Plumbing*

|  |  |
| --- | --- |
| **Project Type** | **Graywater Sources Requiring Mandatory Dual Drainage Plumbing** |
| **New Construction:**   * Accessory Dwelling Unit (ADU), or * Single-family Dwelling | * At least one clothes washer and * At least one shower or one bathtub shower from the master bathroom |
| **New Construction:**  Duplex Dwelling | * At least one clothes washer in each unit and * At least one shower or one bathtub shower from the master bathroom in each unit |
| **New Construction:**  Multi-family Residential Building  (3 or more dwelling units) | * All common laundry facilities and * All showers in pool and spa area(s) |
| **Bathroom Addition:**   * ADU, * Single-family Dwelling, or * Duplex Dwelling | * One shower or bathtub shower when adding shower or bathtub shower |
| **Bathroom Remodel:**   * ADU, * Single-family Dwelling, or * Duplex Dwelling | * One shower or bathtub shower when altering drainage piping to the shower is part of the remodel project |
| **Laundry Room Addition or Remodel:**   * ADU, * Single-family Dwelling, or * Duplex Dwelling | * Clothes washer |